| Tipro API Communicate with Tipro devices

SpeakerBox104.h
1 /*##PBP DEPLOY*/
2 #pragma once
3 /****************************************************************************/
4 /* SPEAKERBOX 104 DEFINES */
5 /****************************************************************************/
6
7 // available audio outputs
8 #define SBX104_HEADSET_SPEAKER 0x00
9 #define SBX104_EXTERNAL_SPEAKER 0x02
10 #define SBX104_RECORDING_OUTPUT 0x03
11
12 // audio outputs levels
13 #define SBX104_AUDIO_OUTPUT_LEVEL_0 0x00
14 #define SBX104_AUDIO_OUTPUT_LEVEL_1 0x01
15 #define SBX104_AUDIO_OUTPUT_LEVEL_2 0x02
16 #define SBX104_AUDIO_OUTPUT_LEVEL_3 0x03
17 #define SBX104_AUDIO_OUTPUT_LEVEL_4 0x04
18 #define SBX104_AUDIO_OUTPUT_LEVEL_5 0x05
19 #define SBX104_AUDIO_OUTPUT_LEVEL_6 0x06
20 #define SBX104_AUDIO_OUTPUT_LEVEL_7 0x07
21 #define SBX104_AUDIO_OUTPUT_LEVEL_8 0x08
22 #define SBX104_AUDIO_OUTPUT_LEVEL_9 0x09
23 #define SBX104_AUDIO_OUTPUT_LEVEL_10 0x0A
24
25 #define SBX104_AUDIO_OUTPUT_LEVEL_MIN SBX104_AUDIO_OUTPUT_LEVEL_0
26 #define SBX104_AUDIO_OUTPUT_LEVEL_MAX SBX104_AUDIO_OUTPUT_LEVEL_10
27
28 // LEDs
29 #define SBX104_LED_1 0x00 /* LED can not be used by API ( used for 12V detection ) */
30 #define SBX104_LED_2 0x01 /* LED can not be used by API ( used for microphone state indication ) */
31 #define SBX104_LED_3 0x02
32 #define SBX104_LED_4 0x03
33
34 #define SBX104_LED_OFF 0x00
35 #define SBX104_LED_ON 0x01
36
37 // microphone
38 #define SBX104_MIC_ACTIVE 0x00
39 #define SBX104_MIC_MUTE 0x01
40
41 // microphone level
42 #define SBX104_MIC_LEVEL_0 0x00
43 #define SBX104_MIC_LEVEL_1 0x01
44 #define SBX104_MIC_LEVEL_2 0x02
45 #define SBX104_MIC_LEVEL_3 0x03
46 #define SBX104_MIC_LEVEL_4 0x04
47 #define SBX104_MIC_LEVEL_5 0x05
48 #define SBX104_MIC_LEVEL_6 0x06
49 #define SBX104_MIC_LEVEL_7 0x07
50 #define SBX104_MIC_LEVEL_8 0x08
51 #define SBX104_MIC_LEVEL_9 0x09
52 #define SBX104_MIC_LEVEL_10 0x0A
53 #define SBX104_MIC_LEVEL_11 0x0B
54 #define SBX104_MIC_LEVEL_12 0x0C
55 #define SBX104_MIC_LEVEL_13 0x0D
56 #define SBX104_MIC_LEVEL_14 0x0E
57
58 #define SBX104_MIC_LEVEL_MIN SBX104_MIC_LEVEL_0
59 #define SBX104_MIC_LEVEL_MAX SBX104_MIC_LEVEL_14
60
61 // microphone pre-amplifer level
62 #define SBX104_MIC_PRE_AMP_LEVEL_0 0x00
63 #define SBX104_MIC_PRE_AMP_LEVEL_1 0x01
64 #define SBX104_MIC_PRE_AMP_LEVEL_2 0x02
65 #define SBX104_MIC_PRE_AMP_LEVEL_3 0x03
66 #define SBX104_MIC_PRE_AMP_LEVEL_4 0x04
67 #define SBX104_MIC_PRE_AMP_LEVEL_5 0x05
68 #define SBX104_MIC_PRE_AMP_LEVEL_6 0x06
69 #define SBX104_MIC_PRE_AMP_LEVEL_7 0x07
70 #define SBX104_MIC_PRE_AMP_LEVEL_8 0x08
71 #define SBX104_MIC_PRE_AMP_LEVEL_9 0x09
72 #define SBX104_MIC_PRE_AMP_LEVEL_10 0x0A
73
74 #define SBX104_MIC_PRE_AMP_LEVEL_MIN SBX104_MIC_PRE_AMP_LEVEL_0
75 #define SBX104_MIC_PRE_AMP_LEVEL_MAX SBX104_MIC_PRE_AMP_LEVEL_10
76
77
78 // compression settings
79 #define SBX104_MIC_COMPRESSION_OFF 0x10
80 #define SBX104_MIC_COMPRESSION_ON 0x11
81 #define SBX104_MIC_COMPRESSION_ILLEGAL 0xFF
82
83
84 // noise threshold
85 #define SBX104_MIC_THRESHOLD_VERY_LOW 0x10
86 #define SBX104_MIC_THRESHOLD_LOW 0x11
87 #define SBX104_MIC_THRESHOLD_MID 0x12
88 #define SBX104_MIC_THRESHOLD_HIGH 0x13
89 #define SBX104_MIC_THRESHOLD_ILLEGAL 0xFF
90
91 #define SBX104_MIC_THRESHOLD_MIN SBX104_MIC_THRESHOLD_VERY_LOW
92 #define SBX104_MIC_THRESHOLD_MAX SBX104_MIC_THRESHOLD_HIGH